MBOX-Line: From arnt at gulbrandsen.priv.no  Thu May 19 00:49:18 2005
To: imap-protocol@u.washington.edu
From: Arnt Gulbrandsen <arnt@gulbrandsen.priv.no>
Date: Fri Jun  8 12:34:36 2018
Subject: [Imap-protocol] BINARY.SIZE for a multipart
In-Reply-To: <7B822F730F822147977ED5B684ACE490241504@xmb-sjc-21b.amer.cisco.com>
References: <7B822F730F822147977ED5B684ACE490241504@xmb-sjc-21b.amer.cisco.com>
Message-ID: <QfUp/SCMRFPLnvUgJnBShw.md5@prosecco.oryx.com>

In RFC 3516, the one problem I ran into was the meaning of BINARY.SIZE 
for bodyparts that don't have an encoding, i.e. Content-Type: 
multipary/*, message/rfc822 or message/external.

Any opinions about the right BINARY.SIZE for such things?

Arnt

