MBOX-Line: From rfs9999 at earthlink.net  Fri Oct  7 07:30:57 2011
To: imap-protocol@u.washington.edu
From: Rick Sanders <rfs9999@earthlink.net>
Date: Fri Jun  8 12:34:46 2018
Subject: [Imap-protocol] FETCH (rfc822) response
In-Reply-To: <alpine.OSX.2.00.1107292242400.911@hsinghsing.panda.com>
References: <4DEBB242.2090200@BusCom.net>
	<alpine.OSX.2.00.1106051606130.4942@hsinghsing.panda.com>
	<4E3382E3.3010509@earthlink.net>
	<alpine.BSO.2.00.1107292118540.19142@morgaine.smi.sendmail.com>
	<alpine.OSX.2.00.1107292242400.911@hsinghsing.panda.com>
Message-ID: <4E8F0D21.3040004@earthlink.net>

I'm working with a server whose response to a FETCH (rfc822) is 
different than I have seen before.

 >> 1 FETCH 1 (rfc822)
<< * 1 EXISTS
<< * 1 FETCH (RFC822[] {0}

I'm used to seeing something like * 1 FETCH (RFC822 {1522}.  In this 
case I have to send a separate 1 FETCH 1 (rfc822.size) command to get 
the message size:   << 1 FETCH (rfc822.size 5149).

Just curious, is this compliant?

-Rick

